# Design Rule Verification Report

Date: |  | 21/11/2024
Time: |  | 10:49:52
Elapsed Time: |  | 00:00:01
Filename: |  | C:\travail\OCEANPHYSICS\2021\POWER_DISTRIB\08 - project\POWERDISTRIB-2024.PcbDoc
Warnings: |  | 0
Rule Violations: |  | 0

## Summary

Warnings | Count
--- | ---
Total | 0

Rule Violations | Count
--- | ---
Clearance Constraint (Gap=0.254mm) (All),(All) | 0
Clearance Constraint (Gap=0.5mm) (InPolygon),(All) | 0
Short-Circuit Constraint (Allowed=No) (All),(All) | 0
Un-Routed Net Constraint ( (All) ) | 0
Modified Polygon (Allow modified: No), (Allow shelved: No) | 0
Width Constraint (Min=0.254mm) (Max=15mm) (Preferred=1mm) (All) | 0
Power Plane Connect Rule(Relief Connect )(Expansion=0.508mm) (Conductor Width=0.254mm) (Air Gap=0.254mm) (Entries=4) (All) | 0
Hole Size Constraint (Min=0.025mm) (Max=10mm) (All) | 0
Hole To Hole Clearance (Gap=0.254mm) (All),(All) | 0
Minimum Solder Mask Sliver (Gap=0.254mm) (Disabled)(All),(All) | 0
Silk To Solder Mask (Clearance=0.254mm) (Disabled)(IsPad),(All) | 0
Silk to Silk (Clearance=0.254mm) (Disabled)(All),(All) | 0
Net Antennae (Tolerance=0mm) (All) | 0
Room 1 (Bounding Region = (0mm, 0mm, 50.8mm, 25.4mm) (Disabled)(InComponentClass('1')) | 0
Room 2 (Bounding Region = (0mm, 0mm, 50.8mm, 25.4mm) (Disabled)(InComponentClass('2')) | 0
Height Constraint (Min=0mm) (Max=25.4mm) (Prefered=12.7mm) (Disabled)(All) | 0
Silk primitive without silk layer | 0
Total | 0